Copyright 2023

Metal Roof Innovations, Ltd.

**ColorGard – Continuous/Fence, Color-Matching System**

[www.S-5.com](http://www.S-5.com)

(turn on Hidden Text)

**SECTION 07 72 53**

**SNOW GUARDS**

This section has been prepared by Metal Roof Innovations, Ltd. for use in the preparation of a project specification. Attachment may be by one of the following methods:

S-5! Clamps: A non-penetrating system for use on standing seam metal roofs.

VersaBracket and VersaGard: A face-fastened (penetrating) system for use on exposed-fastened metal panels, metal tiles and shingles, and selected other roof types.

SnoBracket: A face-fastened (penetrating) system for use on exposed-fastened, trapezoidal-ribbed insulated metal panel (IMP) roofs to prevent thermal bridging. Compatible with ColorGard.

S-5! offers **multiple** fence type snow guards to meet the needs of various projects. (https://s-5.com/products/snow-retention/)

PLEASE NOTE: In 1992, S-5! pioneered a distinctive category of engineered manufactured metal roof attachments. S-5! products are engineered; third party ISO 17025 tested; published holding strengths; the only company in our category recognized by ICC ES (ESR-3869); all products come with limited lifetime materials and manufacturer warranty; a limited lifetime system performance warranty on ColorGard, which covers installation; see (https://s-5.com/warranty/)

The following should be noted in using this specification:

Hypertext links to specific websites are included after manufacturer names and names of organizations whose standards are referenced within the text, to assist in product selection and further research. Hypertext links are contained in parenthesis, e.g.: ([www.S-5.com](http://www.S-5.com))

Optional text requiring a selection by the user is enclosed within brackets, e.g.: "Section [09 00 00.] [\_\_\_\_\_.]"

Items requiring user input are enclosed within brackets, e.g.: "Section [\_\_\_\_\_ - \_\_\_\_\_\_\_\_]."

Optional paragraphs are separated by an "OR" statement, e.g.: \*\*\*\* OR \*\*\*\*

"Green" requirements are included for projects requiring LEED certification, and are included as green text. For additional information on LEED, visit the U.S. Green Building Council website at [www.usgbc.org](http://www.usgbc.org).

For assistance on the use of the products in this section, contact Metal Roof Innovations, Ltd. by calling 888-825-3432, by emailing architecturalsales@s-5.com, support@s-5.com or by visiting our website at [www.S-5.com](http://www.S-5.com).

1. **- GENERAL**

1.1 SUMMARY

Edit the following paragraphs to include only those items specified in this section.

* + 1. Section Includes:
			1. Snow guards for metal roofs.
			2. **[Non-penetrating] [Face-fastened]** attachment system.
	1. RELATED SECTIONS

Coordinate the following paragraphs with other sections in the project manual.

 A. Division 01: Administrative, procedural and temporary work requirements apply to this section.

B. Section 07 41 13 – Metal Roof Panels

C. Section 07 61 00 – Sheet Metal Roofing

D. Section 07 62 00 – Sheet Metal Flashing and Trim

1. Section 07 72 53 – Roof Accessories – Snow Guards

F. Section 13 34 19 – Metal Building Systems

* 1. REFERENCES
		1. Aluminum Association (AA) ([www.aluminum.org](http://www.aluminum.org)) - Aluminum Standards and Data, Current Edition.
		2. ASTM International (ASTM) ([www.astm.org](http://www.astm.org)):
			1. A484/A484M-16 – Standard Specifications for General Requirements for Stainless Steel Bars, Billets and Forgings.
			2. A554-16 – Standard Specification for Welded Stainless Steel Mechanical Tubing.
			3. A555/A555M-16 – Standard Specification for General Requirements for Stainless Steel Wire and Wire Rods.
			4. B85-03 – Standard Specification for Aluminum-Alloy Die Castings.
			5. B221-04a – Standard Specification for Aluminum and Aluminum-Alloy Extruded Bars, Rods, Wire, Profiles and Tubes.
			6. F836M-02 (Current) – Standard Specification for Style 1 Stainless Steel Metric Nuts (Metric).
			7. F880-12 – Standard Specification for Stainless Steel Socket, Square Head, Torx and Slotted Headless-Setscrews.
		3. ICC Evaluation Service ([www.icc-es.org](http://www.icc-es.org)):
			1. Division: 05 00 00 – METALS; Section: 05 05 23 – METAL FASTENERS Evaluation Report ESR-3869.
		4. IAPMO Uniform Evaluation Services
			1. IAPMO UES EC 029-2018; Division: 05 00 00 – METALS; 05 05 23 METAL FASTENINGS; UES Evaluation Report Number: 805
	2. SUBMITTALS

Limiting submittals to only those actually required helps to minimize liability arising from the review of submittals. Minimize submittals on smaller, less complex products.

Include the following for submission of shop drawings, product data and samples for the Architect's review:

S-5! offers a web-based snow calculator to produce engineered calculations for submission. (https://s-5.com/snow-calculator/) Wet stamp by third-party PE available.

* + 1. Action Submittal:
			1. Shop Drawings: Include roof plans showing locations of snow guards on roof and attachment details and spacing.
			2. Product Data:
				1. Product description.
				2. Construction details.
				3. Material descriptions.
				4. Individual component dimensions.
				5. Finishes.
				6. Installation instructions.
			3. Samples:
				1. **[Clamp][Bracket]** samples.
				2. 12-inch long cross member samples including all associated hardware.
		2. Informational Submittals:
			1. Proof of Job Specific Engineering: Include registered professional engineer wet-stamped calculation for number and frequency of snow guard attachments based on designed roof snow load, roof slope, roof dimensions, specific roof profile name, material type, gauge thickness and brand of manufacture; brand and model of snow retention device. **[(https://s-5.com/snow-calculator/)]**
			2. Proof of Product Testing: Results of appropriate product tensile load testing, issued by a recognized ISO 17025 accredited independent testing laboratory, showing the mean (of a minimum three test pulls) ultimate load-to-failure value of attachment **[bracket] [clamping device]** proposed on the specimen material named in B.1.
			3. Proof of Certified Production: Copy of manufacturer current ISO 9001 certificate (latest edition).
			4. Proof of Best Practice Compliance: Manufacturer duly executed letter stating full compliance with all provisions of the Metal Construction Association technical bulletin, “Qualifying Snow Retention Systems for Metal Roofing” (latest edition).

Include the following for submission of closeout submittals for the Owner’s record purposes.

* + 1. Closeout Submittals:
			1. Certification: Installer's certification or duly executed letter stating snow guard system was installed in accordance with manufacturer's instructions and approved shop drawings.
	1. QUALITY ASSURANCE
		1. Manufacturer Qualifications: Manufacturer to specialize in production of snow guard products of the type specified with a minimum of 10 years documented experience.
		2. Manufactured in an ISO 9001 (current) certified facility; ICC audited facility.
		3. Installer Qualifications: Installer to specialize in metal roof installation and installation of snow guard products with a minimum of 5 years documented experience.

Include the following for full-size mockups for review of construction and coordination of work of several sections.

* + 1. Mockup:
			1. Size: Minimum **[8] [\_\_]** feet long.
			2. Show: Snow guard attachment, cross members, and accessories.
			3. Locate **[where directed] [\_\_\_\_]**.
			4. Approved mockup may remain as part of the Work.

Include E.2 for roofs using S-5! ColorGard. System Performance Warranty available for an additional cost, which includes inspections to verify proper installation, and covers system as installed. Lifetime of roof or 30 years--whichever comes first. (s-5.com/warranty/)

* + 1. Warranty:
			1. Lifetime material/workmanship warranty on all products.
			2. System performance warranty.
	1. DELIVERY, STORGE AND HANDLING
		1. Deliver components to jobsite properly packaged to provide protection during transport, delivery and handling.
		2. Store products in manufacturer’s original labeled and unopened packaging in a clean and dry location, protected from potential damage, until ready for application.
1. **- PRODUCTS**
	1. SYSTEM DESCRIPTION

Include the following for snow guards installed using S-5! clamps on standing seam roofs only.

* + 1. Attachment system to provide attachment to standing seam metal roofs:
			1. With dimpling deformation of panel seams only at setscrew locations.
			2. Without penetrations through roof seams or panels.
			3. Without use of sealants or adhesives.
			4. Without violation of roof warranty.

\*\*\*\*OR\*\*\*\*

Include the following for snow guards installed using S-5! brackets on exposed-fastened and exposed-fastened insulated metal panel (IMP) roofs only.

* + 1. Attachment system to provide attachment to **[trapezoidal] [corrugated]** exposed-fastened metal roofs:
			1. Factory-applied butyl sealant.
			2. Without use of sealants or adhesives.

Roof snow loads expected for any given project vary based on project location, roof dimensions, roof slope, wind effects and building configuration. The following paragraph establishes the minimum in-service vector load(s) in pounds per linear foot of eave, which is then used to design the attachment system. This vector load must be determined from the site-specific details by a structural engineer or in conjunction with the S-5! distributor and/or S-5! snow calculator (https://s-5.com/snow-calculator/). Note, the in-service vector load is not the same as the code-dictated snow load based on horizontal at-grade surfaces. Note to see structural drawings for roof snow load.

B. Performance Requirements: Provide snow guards to withstand exposure to the weather and environmental elements and resist design forces without failure due to defective material or manufacture.

1. Loading: Design snow guard system to resist minimum design roof snow load(s) **[of \_\_.] [See structural drawings for roof design snow loads.]**

1. Factor of Safety: Utilize a factor of safety ≥ **[2] [\_\_\_\_]** to determine allowable loads from ultimate tested **[clamp][bracket]** tensile mean load values.

3. Source Limitation: Provide snow guard system as designed and tested by the manufacturer as a complete system. Install all system components by the same manufacturer.

* 1. MANUFACTURER
		1. Basis of Design: S-5!® div. of Metal Roof Innovations, Ltd., 500 W. Highway St., Iowa Park, TX 76367; Tel: 888-825-3432; Fax: 719-495-0045; Email: support@s-5.com; Web: www.s-5.com [(www.S-5.com](http://www.S-5.com))
		2. Acceptable Manufactures if products meet specification requirements:
			1. S-5!® div. of Metal Roof Innovations, Ltd. <https://www.s-5.com/>
			2. LMCurbs. <https://www.lmcurbs.com/>
			3. Rocky Mountain Snow Guards Inc. <https://www.rockymountainsnowguards.com/>

Edit the following to indicate whether or not substitutions will be permitted for the products in this section.

* + 1. Substitutions: [Under provisions in Division 1.] Not permitted.
	1. CONTINUOUS, COLOR-MATCHING – TYPE SNOW RETENTION SYSTEMS FOR **[STANDING SEAM] [EXPOSED-FASTENED] [EXPOSED-FASTENED, TRAPEZOIDAL-RIBBED INSULATED METAL PANEL]** METAL ROOFS

Include the following for roofs using S-5! non-penetrating attachment clamps. Do not use S-5! Mini Clamps for the attachment of ColorGard.

A. Basis of Design: ColorGard®, manufactured by S-5! div. of Metal Roof Innovations, Ltd.

B. Components:

* + - 1. Clamps:

a. Manufactured from 6000-series aluminum extrusions conforming to ASTM B221 or aluminum castings conforming to ASTM B85 and to AA Aluminum Standards and Data.

1) Clamp model to be as recommended by the manufacturer for the specific seam profile used on the project.

b. Setscrews: 300-series stainless steel, 18-8 alloy, 3/8 inch (9.525 mm) diameter, with round nose point.

c. Attachment bolts: 300-series stainless steel, 18-8 alloy, 8 mm diameter, hex flange bolt.

\*\*\*\*OR\*\*\*\*

Include the following for exposed fastened metal panels or metal tiles and shingles using a face-fastened (penetrating) attachment. VersaBracket is designed for trapezoidal exposed-fastened metal roofs; CorruBracket is designed for exposed-fastened corrugated metal roofs; SnoBracket is designed for exposed-fastened trapezoidal-ribbed IMP metal roofs.

2. Brackets:

* + - * 1. Manufactured from 6000-series alloy and temper-aluminum extrusions conforming to ASTM B221 and AA Aluminum Standards and Data.

Model: **[VersaBracket 47.] [VersaBracket 67.] [CorruBracket.] [SnoBracket.]**

The following screws are available (not included) by S-5! div. of Metal Roof Innovations, Ltd. Screws must be compatible with VersaBracket. (Screws provided with SnoBracket)

* + - * 1. Screws for attachment of brackets to roof: as specifically tested to the substrate used on the project, and furnished by snow guard manufacturer. All fastener portions exposed to the weather shall be stainless steel or Zinc/Aluminum cap.

3. Cross Members:

* + - * 1. Manufactured from 6000-series alloy and temper-aluminum extrusions conforming to ASTM B221 and AA Aluminum Standards and Data.
				2. Receptacle in face to receive color-matched metal strips.
				3. Provide splice connectors ensuring alignment and structural continuity at end joints.

4. Color Strips: Same material and finish as roof panels; obtained from roof panel manufacturer.

Snow and ice clips are recommended at eaves for standing seam roofs with seam heights of 2 inches (50.8 mm) or more and are optional for seam heights less than 2 inches (50.8 mm). Recommended on row closest to the eave when specified.

1. Snow and Ice Clips:
	* + - 1. Aluminum, with rubber foot extending to and resting at surface of metal panels; minimum 3 inches (76.2 mm) wide.

 1) Model: SnoClip II or SnapClip II for standing seam heights 1 inch (25.4mm) to 1.5 inches (38.1 mm).

 2) Model: SnoClip III or SnapClip III for standing seam heights 1.75 inches (44.45 mm) to 3.25 inches (82.55 mm).

**PART 3- EXECUTION**

* 1. EXAMINATION

Include the following for roofs using S-5! attachment.

A. Prior to beginning installation, verify:

1. Panel seaming is complete.

2. Panel attachment is sufficient to withstand loads applied by snow guard system.

3. Installation will not impeded roof drainage.

\*\*\*\* OR \*\*\*\*

Include the following for exposed-fastened metal roofs including insulated metal panel exposed-fastened metal roofs.

B. Prior to beginning installation, verify:

1. Roof attachment is sufficient to withstand loads applied by snow guard system.

* + - 1. Installation will not impede roof drainage.
	1. PREPARATION
		1. Clean areas to receive attachments; remove loose and foreign matter that could interfere with installation or performance.

Include the following for roofs using VersaBracket, VersaGard, CorruBracket or SnoBracket attachment.

* + 1. Wipe away excess oil and debris at bracket locations.

Include the following for roofs using S-5! clamp attachment. Always install in accordance with the manufacturer’s instructions: (https://www.s-5.com/products/colorgard/#downloads)

3.3 INSTALLATION

1. Install system in accordance with manufacturer's instructions and approved shop drawings.

B. ColorGard snow retention system:

* + - 1. Place clamps at maximum 32 inches (812.6 mm) on center or as required by certified calculation.
			2. Place clamps in straight, aligned rows using a string line.
			3. Place both setscrews on same side of clamp.
			4. Tighten setscrews to manufacturer's recommended torque. Calibrate tool to setscrew torque using calibrated dial-indicating torque wrench.
			5. Insert color-matched metal strips into cross members, staggering strips to cover cross-member joints.
			6. Attach cross members to clamps; tighten bolts to manufacturer's recommended torque.
			7. Install splice connectors at cross-member end joints.
			8. Do not cantilever cross members more than 8 inches (203.2 mm) beyond last clamp at assembly ends.

Include the following when applicable. Use one SnoClip or SnapClip per panel for panels up to and including 24 inch seam spacing and two per panel over 24 inches. Recommended on row closest to the eave when specified.

* + - 1. Install SnoClips or SnapClips at spacings indicated on shop drawings.
				1. SnoClips: slide onto cross member before securing cross member to clamps.
				2. SnapClips: Secure clips to back side of the cross member using stainless steel #10 x ½ inch (12.7 mm) screw provided.

\*\*\*\* OR \*\*\*\*

Include the following for roofs using thru fasten bracket attachment. [VersaBracket 67], [VersaBracket 47], [Corrubracket]

* + - 1. Place brackets at maximum 32 inches (812.6 mm) on center or as required by certified calculation.
			2. Clean roof area to receive bracket. Remove protective seal on butyl tape.
			3. Place brackets in straight rows along underlying substrate using a string line.
			4. Insert color-matched metal strips into cross members.
			5. Place brackets at spot of attachment. Fasten with screws best suited for type of attachment, and install according to the manufacturer’s instructions.
			6. Attach cross members to brackets using self drilling screws.
			7. Install splice connectors at cross-member end joints.
			8. Do not cantilever cross members more than 8 inches (203.2 mm) beyond last bracket at assembly ends.

Include the following when applicable. Use one SnoClip or SnapClip per panel for panels up to and including 24 inch seam spacing and two per panel over 24 inches. Recommended on row closest to the eave when specified.

* + - 1. Install SnoClips or SnapClips at spacings indicated on shop drawings.
				1. SnoClips: slide onto cross member before securing cross member to clamps
				2. SnapClips: Secure **[SnapClip II] [SnapClip III]** to back side of cross member using stainless steel #10 x ½ inch (12.7 mm) screw (provided).

Include the following for roofs using the SnoBracket; a face-fastened (penetrating) attachment used to attach ColorGard to exposed-fastened IMP using VersaClip. See manufacturer’s instructions..

* + - 1. Place brackets at maximum 32 inches (812.6 mm) on center or as required by certified calculation.
			2. Clean roof area to receive bracket. Remove protective seal on butyl tape.
			3. Place brackets in straight rows along underlying substrate using a string line. Orient the bolt hole downslope.
			4. Secure the bracket directly to the rib of the panel, straddling the profile.
			5. Secure the SnoBrackets by driving the provided fasteners into the pre-punched holes. All eight pre-punched holes must be used to achieve published tested strength. Drive fasteners in until they are tight and the washer is firmly seated. Do not overdrive fasteners.
			6. Install the ColorGard system using Versaclips with provided M8 bolts.
			7. Be sure not to cantilever more than 8 inches beyond the last bracket. Any trimmed piece of ColorGard must be attached with at least two clamps.
			8. Insert color-matched metal strips into cross members.
			9. Install splice connectors at cross-member end joints.
			10. Install SnoClips or Snapclips at designated spacings indicated on shop drawings.
				1. SnoClips: slide onto cross member before securing cross member to clamps.
				2. SnapClips: Secure clips to back side of the cross member using stainless steel #10 x ½ inch (12.7 mm) screw provided.

END OF SECTION